For 1990-2009 cars

### Removal Procedure

1. Remove the window from the front side door. Refer to Front Side Door Window Replacement .
2. Remove the 6 regulator screws (1, 2).
3. Slide the regulator through the large opening in the inner door panel. Remove the regulator from the vehicle.

### Installation Procedure

1. Apply a multipurpose grease to all lubrication and sliding points.
2. Install the regulator through the large opening in the inner door panel.
3. Install the regulator to the door. Secure the regulator with the 6 screws (1, 2).
4. Install the window to the front side door. Refer to Front Side Door Window Replacement .