For 1990-2009 cars

### Removal Procedure

1. Open the rear side door.
2. Open the rubber cap (3) in order to gain access to the door jamb switch retaining screw (2).
3. Remove the retaining screw (2) which secures the door jamb switch (1) to the door jamb.
4. Disconnect the door jamb switch electrical connector (1).
5. Remove the door jamb switch (2) from the vehicle.

### Installation Procedure

1. Connect the door jamb switch electrical connector (1).
2. Install the door jamb switch (1) to the door jamb. Secure the switch with the retaining screw (2).
3. Close the rubber cap (3).
4. Close the rear side door.