For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Travel | 55-85 mm with 30 kg or 294 N of force | 2.18-3.36 in with 66 lbs of force
Push Rod Clevis Length | 109.5-110.5 mm | 4.31-4.35 in
Stoplamp Switch-to-Brake Pedal Clearance | 1.5-2.0 mm | 0.06-0.08 in
Distance from the Booster Piston Rod to the Mating Surface of the Booster

- 1.6L Non-ABS

9.40-9.62 mm

0.370-0.378 in