For 1990-2009 cars

### Right Side Removal Procedure

1. Gently pry and release the tabs on the top of the right air outlet.
2. Remove the right air outlet (6) from the instrument panel (IP).

### Right Side Installation Procedure

1. Align the right air outlet (6) with the duct and install to the IP.
2. Snap the right air outlet into place.

### Left Side Removal Procedure

1. Remove the IP cluster bezel. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement in Instrument Panel, Gages and Console.
2. Gently pry and release the tabs on the top of the left air outlet.
3. Remove the left air outlet (10) from the IP.

### Left Side Installation Procedure

1. Align the left air outlet (10) with the duct and install to the IP.
2. Snap the left air outlet into place.