For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank from the vehicle. Refer to Fuel Tank Replacement .
2. Disconnect the fuel tank pressure sensor electrical connector.
3. Remove the two bolts (1) and the fuel tank pressure sensor (2) from the fuel tank.

### Installation Procedure

Important: Install the fuel tank pressure sensor to the fuel tank with the sensor terminals facing the fuel level sensor (gauge) side.

1. Install the fuel tank pressure sensor (2) to the fuel tank.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the fuel tank pressure sensor with the two bolts (1).

Tighten
Tighten the two fuel tank pressure sensor bolts to 1.2 to 2.0 N·m (11 to 18 lb in).

3. Connect the fuel tank pressure sensor electrical connector.
4. Install the fuel tank to the vehicle. Refer to Fuel Tank Replacement .