For 1990-2009 cars

## Front Side Door Lower Molding Replacement LT Models

### Removal Procedure

1. Use a taped flat bladed tool or a taped trim tool in order to release the 12 plastic retainers that retain the front door lower molding (2). Release the front door lower molding beginning at the bottom of the molding.
2. Remove the front door lower molding (2) from the vehicle.
3. Remove the 12 plastic retainers from the front door and/or the door lower molding (2).

### Installation Procedure

1. Install the 12 plastic retainers to the front door lower molding (2). Replace any retainers that were damaged in the removal process.
2. Install the front door lower molding (2) to the front door. Make certain that the plastic retainers are completely engaged.