For 1990-2009 cars

Listed below are the vehicle inspections and services that should be made by either the owner or a qualified technician at the frequencies indicated to help ensure the following:

• | Proper safety of the vehicle.

• | The vehicle emission system performance.

• | Dependability of the vehicle.

Complete any necessary repairs at once. Use the proper fluids or lubricants whenever adding to the vehicle. For information on fluids and lubricants to use when service is required, refer to Fluid and Lubricant Recommendations .

For emission system diagnosis information, refer to Engine Controls - 1.6 L or Engine Controls - 2.0 L.

For additional Checks and Services, refer to Owner Checks and Services .

### At Each Engine Oil Change

#### Radiator and Heater Hose Inspection

Inspect the hoses and have them replaced if they are cracked, swollen or deteriorated. Inspect all pipes, fittings and clamps. Replace these parts as needed.

#### Throttle Linkage Inspection

Notice: Do NOT lubricate accelerator or cruise control cables. Lubrication will destroy the protective coating on these cables.

Inspect for the following and replace as needed:

1. Missing parts such as retainers or clips.
2. Interference of linkage or cable conduit to critical components such as fuel lines, brake pipes or harness leads.
3. Proximity of cable to exhaust system and other heat sources (check for melting and/or discoloration).
4. Cable kinking, avoid sharp blends of cables.
5. Clearance of throttle system moving parts throughout their travel from other stationary components.
6. Damage of components due to cable kinking, severe abrasion or misalignment.
7. Do not lubricate the accelerator and cruise control cables. Lubricating destroys the protective coating on the cables.

#### Clutch System Service

Inspect clutch pedal free travel and adjust as necessary.

### At Least Twice A Year

#### Automatic/Manual Transmission Check

Inspect the automatic or manual transmission fluid level. Add the proper transmission fluid if needed. A fluid loss may indicate a problem. Inspect the system and repair if needed.

For the automatic transmission fluid level checking procedure, refer to Transmission Fluid Check in Automatic Transmission - 4 Speed - M41.

For the manual transmission fluid level checking procedure, refer to Transmission Fluid Inspection in Manual Transmission - M59 (Tracker).