For 1990-2009 cars

### Removal Procedure

1. Release the 4 retaining clips (2) on the air cleaner cover.
2. Disconnect the evaporative emission (EVAP) system vent hose from the air cleaner cover.
3. Lift the air cleaner cover (1).
4. Remove the air filter element (2).

### Installation Procedure

1. Install the air filter element into the air cleaner box.
2. Install the air cleaner cover.
3. Secure the air cleaner cover with the retaining clips (2).
4. Connect the EVAP system vent hose to the air cleaner cover.