For 1990-2009 cars

Operation | Service Allowed | Service Preferred
--- | --- | ---
Front
Caster (non-adjustable, for reference only) | +1.67° to +3.67° | +2.67°
Cross Caster (non-adjustable, for reference only) | 0.0° to +0.75° | 0.0°
Camber (non-adjustable, for reference only) | -1.00° to +1.00° | 0.0°
Cross Camber (non-adjustable, for reference only) | 0.0° to +0.75° | 0.0°
Toe | +0.08° to -0.08° | 0.0°
Total Toe | +0.16° to -0.16° | 0.0°
Inside Turning Angle | 31.5° to 37.5° | 34.5°
Outside Turning Angle | 29.5° to 35.5° | 32.5°