For 1990-2009 cars

### Removal Procedure

1. Remove the rear floor console. Refer to Rear Floor Console Replacement .
2. Remove the 2 screws and the 2 plastic retainers which secure the front floor console.
3. Lift the console.
4. Disconnect the power/normal switch electrical connector, if equipped with the 4-speed A/T.
5. Remove the front floor console from the vehicle.

### Installation Procedure

1. Connect the power/normal switch electrical connector, if equipped with the 4-speed A/T.
2. Install the front floor console to the vehicle. Secure the console with the 2 screws and the 2 plastic retainers.
3. Install the rear floor console. Refer to Rear Floor Console Replacement .