For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Steering Wheel and Column-Standard Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Steering Wheel and Column - Standard
2 | Verify that the ignition lock cylinder sticks in the START position. Does the ignition lock cylinder stick in the START position? | Go to Step 3 | System OK
3 | Inspect the steering column lock and ignition switch cylinder for damage. Is the steering column lock and ignition switch cylinder damaged? | Go to Step 4 | Go to Step 2
4 | Replace the steering column lock and ignition switch cylinder. Refer to Steering Column Lock and Ignition Switch Cylinder Replacement - On Vehicle . Did you complete the repair? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 2