For 1990-2009 cars

### Removal Procedure

1. Remove the Instrument Cluster Assembly (2). Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console.
2. Remove the Lamp Driver Module (LDM) (1) from the printed circuit.

### Installation Procedure

1. Install the LDM (1) to the printed circuit.
2. Install the Instrument Cluster Assembly (2). Refer to Instrument Cluster Replacement in Instrument Panel, Gages and Console.
3. Perform Diagnostic System Check - ABS .