For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning (A/C) Flexible Hose Bolts | 15 N·m | 11 lb ft
Air Conditioning (A/C) Mounting Bracket Bolts | 23 N·m | 17 lb ft
Battery Cable-to-Battery Terminal Retainers | 15 N·m | 11 lb ft
Cooling Fan Nuts | 11 N·m | 97 lb in
Coolant Intake Pipe Bolt | 11 N·m | 97 lb in
Crankshaft Pulley Bolts | 16 N·m | 12 lb ft
Engine Oil Level Indicator Tube Mounting Bolt | 11 N·m | 97 lb in
Fan Clutch Nuts | 11 N·m | 97 lb in
Generator Mounting Bracket Bolt | 23 N·m | 17 lb ft
Generator Upper Mounting Bolt | 27 N·m | 20 lb ft
Heater Outlet Line Bolt | 15 N·m | 11 lb ft
Outlet Support Pipe Bolt | 11 N·m | 97 lb in
Power Steering Fluid Reservoir Bolts | 15 N·m | 11 lb ft
Radiator Bolts | 10 N·m | 89 lb in
Shroud Bolts | 11 N·m | 97 lb in
Thermostat Cap Bolts | 16 N·m | 12 lb ft
Water Pump Pulley Bolts | 23 N·m | 17 lb ft
Water Pump Nuts and Bolts | 13 N·m | 115 lb in