For 1990-2009 cars

### Right Side Removal Procedure

1. Carefully lift up and pry the right side defroster outlet (5) from the instrument panel (IP).
2. Remove the right side defroster outlet (5) from the IP.

### Right Side Installation Procedure

1. Align the right side defroster outlet (5) with the IP.
2. Snap the right side defroster outlet (5) into place.

### Left Side Removal Procedure

1. Remove the instrument panel (IP). Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.
2. Remove the screw and the left side defroster outlet (1) from the IP.

### Left Side Installation Procedure

1. Install the left side defroster outlet (1) to the IP. Secure with the screw.
2. Install the instrument panel. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.