For 1990-2009 cars

### Removal Procedure

1. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Remove the screws and the door trim support bracket from the door.
3. Peel the water deflector (1) away from the door.
4. Inspect the water deflector (1) for holes.
5. Use waterproof tape in order to repair the holes.
6. Apply waterproof tape to both sides of the water deflector (1), if necessary.

### Installation Procedure

1. Apply adhesive (2) to the back of the water deflector (1).
2. Install the water deflector (1) to the door.
3. Install the door trim support bracket to the door. Secure the bracket with the screws.
4. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .