For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster assembly from the instrument panel. Refer to Instrument Cluster Replacement .
3. Remove all of the bulb sockets from the rear of the instrument cluster assembly (18).
4. Remove all of the screws (1, 2, 3, 4) from the instrument cluster assembly.
5. Remove the instrument cluster printed circuit from the instrument cluster assembly.

### Installation Procedure

1. Install the instrument cluster printed circuit to the instrument cluster assembly. Secure the instrument cluster printed circuit with the screws (1, 2, 3, 4).
2. Install all of the bulb sockets to the rear of the instrument cluster assembly (18).
3. Install the instrument cluster assembly (18) to the instrument panel. Refer to Instrument Cluster Replacement .
4. Connect the negative battery cable.