For 1990-2009 cars

### Removal Procedure

1. Remove the push in retainers from the underside of the rocker panel molding.
2. Slide the rocker panel molding (1) toward the rear of vehicle, in order to disengage from the retaining clips (2).

### Installation Procedure

1. Line up the rocker panel molding (1) to the retaining clips (2), and slide toward the front of vehicle.
2. Install the rocker panel molding push in retainers to the under side of the rocker panel molding.