For 1990-2009 cars

1. Remove the parking brake lever bezel from the vehicle. Refer to Parking Brake Lever Bezel Replacement .
2. Remove the 2 screws and the 2 plastic retaining clips.
3. Lift the console (1).
4. Disconnect the power/normal switch electrical connector, if equipped with 4-speed A/T.
5. Remove the console (1) from the vehicle.

### Installation Procedure

1. Connect the power/normal switch electrical connector, if equipped with 4-speed A/T.
2. Install the console (1) to the vehicle. Secure the console with the 2 screws and the 2 plastic retaining clips.
3. Install the parking brake bezel to the vehicle. Refer to Parking Brake Lever Bezel Replacement .