For 1990-2009 cars

Important: Note the position of the valve lands and sleeves position when assembling the components into their bores.

1. Install the 1-2 accumulator valve spring (505).
2. Install the 1-2 accumulator valves (504).
3. Install the 1-2 accumulator valve plug (503).
4. Install the 1-2 accumulator valve plug retainer pin (502).
5. Install the reverse control valve (513).
6. Install the manual low control valve (512).
7. Install the manual low control valve spring (511).
8. Install the manual low control valve spring retainer pin (502).
9. Install the downshift timing valve spring (510) (low speed).
10. Install the downshift timing valve (509) (low speed).
11. Install the intermediate valve (530).
12. Install the intermediate valve retainer pin (502).
13. Install the downshift timing valve (507) (high speed).
14. Install the downshift timing valve spring (506) (high speed).
15. Install the downshift timing valve spring retainer pin (502).
16. Install the 1-2 shift valve (514).
17. Install the 1-2 shift valve spring (515).
18. Install the 1-2 shift control valve spring (517) onto the control valve (516).
19. Install the 1-2 shift control valve (516) and spring .
20. Install the 1-2 shift control valve sleeve (518).
21. Install the 1-2 shift control valve sleeve retainer pin (502).
22. Install the 2-3 shift valve (519).
23. Install the 2-3 shift control valve spring (521) and seat (520).
24. Install the 2-3 shift control valve (522).
25. Install the 2-3 shift control valve sleeve (523).
26. Install the 2-3 shift control valve sleeve retainer pin (502).
27. Install the 3-2 control valve (524).
28. Install the 3-2 control valve spring (525).
29. Install the 3-2 control valve plug (526).
30. Install the 3-2 control valve spring retainer pin (502).
31. Install the detent pressure regulator valve (527).
32. Install the detent pressure regulator valve spring (528).
33. Install the detent pressure regulator valve spring retainer pin (502).
34. Install the manual valve (138).