For 1990-2009 cars

### Removal Procedure

1. Remove the endgate trim panel seal. Refer to Water Deflector Replacement .
2. Remove the 2 mounting nuts (2) which secure the endgate outside handle.
3. Remove the endgate outside handle (2) from the rear license plate housing (1).

### Installation Procedure

1. Install the endgate outside handle (2) to the rear license plate housing (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the 2 mounting nuts (2) which secure the endgate outside handle.

Tighten
Tighten the endgate outside handle mounting nuts to 10 N·m (89 lb in).

3. Install the endgate trim panel seal. Refer to Water Deflector Replacement .