For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel (IP) compartment.
2. Push in the left and right side of the IP compartment and lower the IP compartment.
3. Release the locking tabs and disconnect the electrical connector.
4. Remove the screw and remove the blower motor relay (3).

### Installation Procedure

1. Install the blower motor relay (3). Secure with the screw.
2. Connect the electrical connector.
3. Close the instrument panel compartment.