For 1990-2009 cars

## Seat Belt Replacement - Center Rear 4 Door

### Removal Procedure

1. Pull the rear seat pull straps (1 and 2) and raise the rear seat cushions (3 and 4) in order to gain access to the rear seat center belt and buckle bolts.
2. Remove the following components from the floor pan (5):

2.1. | The mounting bolt

2.2. | The rear seat center belt (4)

2.3. | The anchor bolt

2.4. | The rear seat belt center buckle (1)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the rear seat center buckle (1) to the floor pan (5). Secure the buckle with the anchor bolt.

Tighten
Tighten the rear seat center buckle anchor bolt to 35 N·m (25 lb ft).

2. Install the rear seat center belt (4) to the floor pan (5). Secure the center belt with the mounting bolt.

Tighten
Tighten the rear seat belt mounting bolt to 35 N·m (25 lb ft).

3. Lower the rear seat cushions (3 and 4).