For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adapter Case Bolts | 36 N·m | 27 lb ft
Brake Apply Cover Bolts | 10 N·m | 89 lb in
Center Support Bolts | 26 N·m | 19 lb ft
Converter Housing Bolt Position A | 36 N·m | 27 lb ft
Converter Housing Bolt Position B | 58 N·m | 43 lb ft
Detent Spring Bolt | 5 N·m | 44 lb in
Fluid Filter Screen Bolts | 5 N·m | 44 lb in
Lower Valve Body Plate Bolts | 5 N·m | 44 lb in
Lower Valve Body Side Bolts | 5 N·m | 44 lb in
Manual Shaft Lever Nut | 13 N·m | 115 lb in
Oil Pump Bolts | 22 N·m | 16 lb ft
Oil Pump Cover-To-Oil Pump Body Bolts | 9 N·m | 80 lb in
Parking Pawl Plate Bolts | 7 N·m | 62 lb in
Pressure Relief Valve Bolts | 5 N·m | 44 lb in
Rear Valve Body Plate Bolts | 5 N·m | 44 lb in
Shift Solenoid Bolts | 10 N·m | 89 lb in
Speed Sensor Bolt | 23 N·m | 17 lb ft
TCC Control Valve Plate Bolts | 5 N·m | 44 lb in
TCC Solenoid Bolts | 5 N·m | 44 lb in
Transmission Oil Pan Bolts | 4 N·m | 35 lb in
Transmission Range Switch Bolt | 5 N·m | 44 lb in
Transmission Range Switch Set Nut | 5 N·m | 44 lb in
TV Cable Cam Bolt | 8 N·m | 71 lb in
Upper Valve Body Side Bolts | 5 N·m | 44 lb in
Valve Body Bolt | 10 N·m | 89 lb in

Application | Specification
--- | ---
Metric | English
Brake Applying Cover Bolts | 10 N·m | 89 lb in
Cooler Pipe Clamp Bolt | 23 N·m | 17 lb ft
Cooler Pipe Flare Nuts | 25 N·m | 18 lb ft
Detent Spring Bolt | 5 N·m | 44 lb in
Engine Rear Mounting Bolts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Engine Rear Mounting Member Bolts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Fluid Cooler Hose Clamps | 1.5 N·m | 12 lb in
Fluid Filler Tube Bracket Bolt | 23 N·m | 17 lb ft
Fluid Filter Screen Bolts | 5 N·m | 44 lb in
Fluid Pressure Switch | 10 N·m | 89 lb in
Flywheel Inspection Cover Bolts | 10 N·m | 89 lb in
Flywheel-to-Torque Converter Bolts | 65 N·m | 48 lb ft
Front Propeller Shaft Bolts and Nuts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Front Skid Plate Bolts | 54 N·m | 40 lb ft
Interlock Cable Nut | 13 N·m | 115 lb in
Left and Right Case Stiffener Bolts | 60 N·m | 44 lb ft
Lower Transmission Retaining Nuts | 85 N·m | 62 lb ft
Lower Valve Body Plate Bolts | 5 N·m | 44 lb in
Lower Valve Body Side Bolts | 5 N·m | 44 lb in
Manual Select Lever Nut | 19 N·m | 14 lb ft
Manual Selector Bolts | 18 N·m | 13 lb ft
Park/Neutral Position Switch Bolt | 21 N·m | 15 lb ft
Pressure Relief Valve Bolts | 5 N·m | 44 lb in
Rear Propeller Shaft Bolts and Nuts | 50 N·m | 37 lb ft
Rear Transmission Crossmember Bolts (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Rear Transmission Mount Bolts (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Rear Valve Body Plate Bolts | 5 N·m | 44 lb in
Shift Lock Solenoid Retaining Bolt | 10 N·m | 89 lb in
Shift Select Cable Locknut | 7 N·m | 62 lb in
Shift Solenoid Assembly Bolts | 10 N·m | 89 lb in
Speedometer Guide Bracket Bold | 9 N·m | 80 lb in
Starter Motor Bolts | 30 N·m | 22 lb ft
Stoplamp Switch Adjustment Nut | 15 N·m | 11 lb ft
TCC Control Valve Plate Bolts | 5 N·m | 44 lb in
TCC Solenoid Retaining Bolts | 5 N·m | 44 lb in
Torque Stopper Bushing Bolts (Four-Wheel Drive Models) | 50 N·m | 37 lb ft
Transfer Adapter Case Bolts | 31 N·m | 23 lb ft
Transfer Plate-to-Valve Body Bolts | 9 N·m | 80 lb in
Transmission Fluid Drain Plug | 17 N·m | 13 lb ft
Transmission Fluid Pan Bolts | 5 N·m | 44 lb in
Transmission Range Switch Bolt | 5 N·m | 44 lb in
Transmission Range Switch Set Nut | 5 N·m | 44 lb in
TV Cable Cam Bolt | 8 N·m | 71 lb in
Upper Transmission Retaining Bolts | 85 N·m | 62 lb ft
Upper Valve Body Side Bolts | 5 N·m | 44 lb in
Valve Body Bolts | 10 N·m | 89 lb in