For 1990-2009 cars

### Removal Procedure

Caution: Halogen bulbs contain gas under pressure. Handling a bulb improperly could cause it to shatter into flying glass fragments. To help avoid personal injury:

• | Turn off the lamp switch and allow the bulb to cool before changing the bulb.

• | Leave the lamp switch OFF until the bulb change is complete.

• | Always wear eye protection when changing a halogen bulb.

• | Handle the bulb only by its base. Avoid touching the glass.

• | Keep dirt and moisture off the bulb.

• | Properly dispose of the used bulb.

• | Keep halogen bulbs out of the reach of children.

1. Disconnect the headlamp bulb electrical connector.
2. Turn the lock ring (4) counterclockwise in order to loosen the headlamp bulb lock ring (4).
3. Pull the headlamp bulb (3) using the lock ring (4) from the headlamp assembly (2).
4. Save the lock ring (4) in order to reuse with the new bulb.

### Installation Procedure

1. Install the headlamp bulb (3) to the headlamp assembly (2).
2. Rotate the lock ring (4) clockwise in order to secure the headlamp bulb (3).
3. Connect the headlamp bulb electrical connector.