For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the hood.
2. Remove the hood front bumper (1) from the vehicle by turning the bumper (1) counterclockwise.

### Installation Procedure

1. Install the hood front bumper (1) to the vehicle by turning the bumper (1) clockwise.
2. Adjust the hood front bumper (1) in order to ensure that the hood is flush with the front fender.
3. Lower the hood.