For 1990-2009 cars

## Side Marker Lamps Inoperative Left

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Exterior Lights Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Lighting Systems
2 | Verify that the left side marker lamp is inoperative. Is the left side marker lamp inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections
3 |

1. Turn the light switch to the ON position.
2. Test for battery voltage at terminal 2 of the left side marker lamp assembly connector.

Is battery voltage present?

Go to Step 5

Go to Step 4

4 | Repair the open in the RED/YEL wire between the left side marker lamp assembly and S217. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 6 | --
5 | Repair the open in the BLK wire between the left side marker lamp assembly and S202. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3

## Side Marker Lamps Inoperative Right

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Exterior Lights Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Lighting Systems
2 | Verify that the right side marker lamp is inoperative. Is the right side marker lamp inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections
3 |

1. Turn the light switch to the ON position.
2. Test for battery voltage at terminal 2 of the right side marker lamp assembly connector.

Is battery voltage present?

Go to Step 5

Go to Step 4

4 | Repair the open in the RED/YEL wire between the right side marker lamp assembly and S217. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 6 | --
5 | Repair the open in the BLK wire between the right side marker lamp assembly and S201. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3