For 1990-2009 cars

## Assist Handle Replacement 2 - Door

### Removal Procedure

1. Remove the assist handle trim covers.
2. Remove the 2 screws (2) which secure the assist handle (1).
3. Remove the assist handle (1) from the vehicle.

### Installation Procedure

1. Install the assist handle (1) to the vehicle. Secure the handle with the 2 screws (2).
2. Install the assist handle trim covers.

## Assist Handle Replacement Rear - 2 Door

### Removal Procedure

1. Remove the assist handle trim covers (3).
2. Remove the 2 screws which secure the assist handle (2).
3. Remove the assist handle (2) from the vehicle.

### Installation Procedure

1. Install the assist handle (2) to the vehicle. Secure the handle with the 2 screws.
2. Install the assist handle trim covers (3).

## Assist Handle Replacement Rear - 4 Door

### Removal Procedure

1. Remove the assist handle trim covers.
2. Remove the 2 screws which secure the assist handle.
3. Remove the assist handle from the vehicle.

### Installation Procedure

1. Install the assist handle to the vehicle. Secure the handle with the 2 screws.
2. Install the assist handle trim covers.