For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Disconnect the actuator pump assembly electrical connector.
3. Remove the bolts (1) and the actuator pump assembly.

### Installation Procedure

1. Install the actuator pump assembly and bolts (1) to the vehicle.
2. Connect the actuator pump assembly electrical connector.