For 1990-2009 cars

## High Mount Stop Lamp Replacement 2 Door

### Removal Procedure

1. Open the rear door.
2. Remove the 2 screws (1) which secure the high mounted stop lamp (2).
3. Pull the stop lamp (3) from the high mounted stop lamp housing (1).
4. Remove the stop lamp bulb socket (2) from the stop lamp (3).
5. Remove the bulb from the socket (2), if necessary.

### Installation Procedure

1. Install the bulb to the socket (2), if removed.
2. Install the high mounted stop lamp bulb socket (2) to the stop lamp (3).
3. Install the stop lamp (3) to the housing (1).
4. Install the 2 screws (1) which secure the stop lamp (2) to the housing.
5. Close the rear door.

## High Mount Stop Lamp Replacement 4 Door

### Removal Procedure

1. Open the rear door.
2. Remove the 2 plastic retainers and the high mounted stop lamp cover (2) from the high mounted stop lamp.
3. Disconnect the high mounted stop lamp electrical connector (2).
4. Remove the following components from the vehicle:

4.1. | The 2 screws (1)

4.2. | The high mounted stop lamp (3)

5. Remove the bulb sockets (4) from the stop lamp (3).
6. Remove the bulbs from the sockets (4), if necessary.

### Installation Procedure

1. Install the bulbs to the sockets (4), if removed.
2. Install the bulb sockets (4) to the high mounted stop lamp (3).
3. Install the high mounted stop lamp (3) to the rear door. Secure the stop lamp with the 2 screws (1).
4. Connect the high mounted stop lamp electrical connector (2).
5. Install the high mounted stop lamp cover (2) to the stop lamp. Secure the cover with the 2 plastic retainers.
6. Close the rear door.