For 1990-2009 cars

### Removal Procedure

1. Remove the folding top bow garnish molding. Refer to Folding Top Bow Garnish Molding Replacement .
2. Remove the following components from the vehicle:

2.1. | The 3 screws

2.2. | The folding top side rail garnish molding (1)

### Installation Procedure

1. Install the folding top side rail garnish molding (1) to the vehicle. Secure the molding with the 3 screws.
2. Install the folding top bow garnish molding. Refer to Folding Top Bow Garnish Molding Replacement .