For 1990-2009 cars

## Rear Door Trim Panel Replacement - Right Side Upper

### Removal Procedure

1. Remove the left rear door upper trim panel (3). Refer to Rear Door Trim Panel Replacement - Left Side .
2. Gently pry the right rear door upper trim panel (1) from the rear door.
3. Remove the high mounted stoplamp wiring harness from the back of the upper trim panel (1).
4. Remove the rear door upper trim panel (1) from the vehicle.

### Installation Procedure

1. Install the high mounted stoplamp wiring harness to the back of the right rear door upper trim panel (1).
2. Install the right rear door upper trim panel (1) to the rear door. Ensure that the plastic retainers are fully engaged.
3. Install the left rear door upper trim panel (3). Refer to Rear Door Trim Panel Replacement - Left Side .