For 1990-2009 cars

## Rear Seat Cushion Replacement 2 Door

### Removal Procedure

1. Gently pry and remove the rear seat hinge support cover (2) from each rear seat hinge support (1).
2. Remove the rear seat stopper rod nut (1) from each rear seat hinge support pin (4).
3. Remove the support pin (4) from each rear seat support (2).
4. Pull the rear seat pull strap (2) while raising the back of the rear seat cushion (1).
5. Remove the seat cushion (1) from the vehicle.

### Installation Procedure

1. Install the rear seat cushion (5) to the vehicle. Secure the cushion to each rear seat support (2) with the rear seat hinge support pins (4).
2. Install the rear seat stopper rod nut (1) to each support pin (4).
3. Install the rear seat hinge support cover (2) to each rear seat hinge support (1).
4. Lower the seat cushion.

## Rear Seat Cushion Replacement 4 Door

### Removal Procedure

1. Gently pry and remove the rear seat hinge support cover (2) from each rear seat hinge support (1).
2. Remove the rear seat stopper rod nut (2) from each rear seat hinge support pin (3).
3. Remove the support pin (3) from each rear seat support.
4. Pull the rear seat pull strap (1 or 2) while raising the back of the rear seat cushion (3 or 4).
5. Remove the seat cushion (3 or 4) from the vehicle.

### Installation Procedure

1. Install the rear seat cushion (1) to the vehicle. Secure the cushion to each rear seat support with the rear seat hinge support pins (3).
2. Install the rear seat stopper rod nut (2) to each support pin (3).
3. Install the rear seat hinge support cover (2) to each rear seat hinge support (1).
4. Lower the seat cushion.