For 1990-2009 cars

### Removal Procedure

1. Lower the front side door window completely.
2. Remove the screw (1) which secures the front side door window outer sealing strip (2).
3. Use a flat-bladed tool wrapped in tape in order to gently pry the outer sealing strip (2) from the front side door (3).

### Installation Procedure

1. Install the front side door window outer sealing strip (2) to the front side door (3) by pressing into place. Secure the strip with the screw (1).
2. Raise the front side door window.