For 1990-2009 cars

## Rear Quarter Trim Panel Replacement 2 Door

### Removal Procedure

1. Remove the folding top side rail garnish molding. Refer to Folding Top Side Rail Replacement in Roof.
2. Remove the folding top #3 bow. Refer to Folding Top Roof Bow Replacement in Roof.
3. Remove the rear quarter trim panel (1) from the vehicle.

### Installation Procedure

1. Install the rear quarter trim panel (1) to the vehicle.
2. Install the folding top #3 bow. Refer to Folding Top Roof Bow Replacement in Roof.
3. Install the folding top side rail garnish molding. Refer to Folding Top Side Rail Replacement in Roof.