For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (IP). Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.
2. Remove the screw and the center air distributor duct (7).
3. Remove the 4 defroster duct screws.
4. Remove the defroster air outlet duct (3) including the left and right defroster air outlets.
5. Remove the IP air outlet duct (11) from the vehicle.

### Installation Procedure

1. Install the IP air outlet duct (11) to the vehicle.
2. Install the defroster air outlet duct (3) including the left and right defroster air outlets (2,4). Secure with the 4 screws.
3. Install the center air distributor duct (7). Secure with the screw.
4. Install the instrument panel. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.