For 1990-2009 cars

### Removal Procedure

1. Remove the rear seatback. Refer to Rear Seat Back Replacement .
2. Unscrew the rear seatback lock knob (15, 2) counterclockwise.
3. Remove the rear seatback lock knob (15, 2) from the seatback (14, 3).
4. Remove the 2 rear seatback seat belt cover screws.
5. Remove the rear seatback seat belt cover.
6. Squeeze the rear seatback hinge sleeve in order to remove the sleeve from the rear seatback side trim.
7. Remove the rear seatback side trim from the rear seatback frame.
8. Cut the 4 hog rings which secure the rear seatback cover to the seat.
9. Remove the seatback cover from the rear seatback frame.

### Installation Procedure

1. Install the rear seatback cover to the rear seatback frame. Secure the rear seatback cover with the 4 hog rings.
2. Install the rear seatback lock knob (2) by turning clockwise in order to secure the lock knob to the seatback.
3. Install the rear seatback side trim to the rear seatback frame.
4. Install the rear seatback hinge sleeve in the rear seatback side trim.
5. Install the rear seatback seat belt cover to the rear seatback frame. Secure the cover with the 2 screws.
6. Install the rear seatback. Refer to Rear Seat Back Replacement .