For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Instrument Cluster Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Instrument Panel, Gages and Console
2 | Verify that the speedometer Indicator is inoperative. Does the speedometer operate normally? | Go to Testing for Intermittent Conditions and Poor Connections | Go to Step 3
3 | Test for an open condition from the instrument cluster connector C1, cavity 5 and battery voltage. Does an open condition exist? | Go to Step 4 | Go to Step 5
4 | Repair the WHT wire from the instrument cluster C1, cavity 5 and the junction block C1, cavity 9. Did you complete the repair? | Go to Step 12 | --
5 | Test for a short to ground condition from the instrument cluster connector C3, cavity 2. Does a short to ground condition exist? | Go to Step 6 | Go to Step 7
6 | Repair the WHT/YEL wire from the instrument cluster C3, cavity 2 and G103. Did you complete the repair? | Go to Step 12 | --
7 | Inspect the instrument cluster printed circuit for any damage or loose connections. Does any damage or loose connections exist? | Go to Step 8 | Go to Step 9
8 | Replace the instrument cluster printed circuit. Refer to Instrument Cluster Replacement Did you complete the repair? | Go to Step 12 | --
9 | Test for an open condition from the instrument cluster connector C1, cavity 9 and the vehicle speed sensor cavity 1. Does an open condition exist? | Go to Step 10 | Go to Step 11
10 | Repair the open condition from the instrument cluster and the VSS. Did you complete the repair? | Go to Step 12 | --
11 | Replace the speedometer. Did you complete the repair? | Go to Step 12 | --
12 | Operate the system in order to verify the repair. Did you complete the repair? | System OK | Go to Step 3