For 1990-2009 cars

## Power Door Locks Actuator Motor Inoperative Rear

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Keyless Entry System Description , Keyless Entry System Operation and Keyless Entry System Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Doors
2 | Verify that the rear door lock is inoperative. Is only the rear door lock inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Disconnect the door lock actuator connector.
2. Connect a test lamp between terminal 2 and ground.

Does the test lamp illuminate with the door lock switch in the LOCK position?

Go to Step 5

Go to Step 4

4 | Repair the open in the BLU wire between the door lock actuator and S308. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
5 | Connect a test lamp between terminal 3 and ground. Does the test lamp illuminate with the door lock switch in the UNLOCK position? | Go to Step 7 | Go to Step 6
6 | Repair the open in the BLU/RED wire between the door lock actuator and S309. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
7 | Replace the door lock actuator. Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3

## Power Door Locks Actuator Motor Inoperative Right Rear

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Keyless Entry System Description , Keyless Entry System Operation and Keyless Entry System Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Doors
2 | Verify that the right rear door lock is inoperative. Is only the right rear door lock inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Disconnect the door lock actuator connector.
2. Connect a test lamp between terminal 2 and ground.

Does the test lamp illuminate with the door lock switch in the LOCK position?

Go to Step 5

Go to Step 4

4 | Repair the open in the BLU wire between the door lock actuator and S308. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
5 | Connect a test lamp between terminal 3 and ground. Does the test lamp illuminate with the door lock switch in the UNLOCK position? | Go to Step 7 | Go to Step 6
6 | Repair the open in the BLU/RED wire between the door lock actuator and S309. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
7 | Replace the door lock actuator. Refer to Rear Side Door Lock Actuator Replacement . Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3

## Power Door Locks Actuator Motor Inoperative Left Rear

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Keyless Entry System Description , Keyless Entry System Operation and Keyless Entry System Circuit Description operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Doors
2 | Verify that the left rear door lock is inoperative. Is only the left rear door lock inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Disconnect the door lock actuator connector.
2. Connect a test lamp between terminal 2 and ground.

Does the test lamp illuminate with the door lock switch in the LOCK position?

Go to Step 5

Go to Step 4

4 | Repair the open in the BLU wire between the door lock actuator and S308. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
5 | Connect a test lamp between terminal 3 and ground. Does the test lamp illuminate with the door lock switch in the UNLOCK position? | Go to Step 7 | Go to Step 6
6 | Repair the open in the BLU/RED wire between the door lock actuator and S309. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
7 | Replace the door lock actuator. Refer to Rear Side Door Lock Actuator Replacement . Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3

## Power Door Locks Actuator Motor Inoperative Right Front

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Keyless Entry System Description , Keyless Entry System Operation and Keyless Entry System Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Doors
2 | Verify that the right front door lock is inoperative. Is only the right front door lock inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Disconnect the door lock actuator connector.
2. Connect a test lamp between terminal 2 and ground.

Does the test lamp illuminate with the door lock switch in the LOCK position?

Go to Step 5

Go to Step 4

4 | Repair the open in the BLU wire between the door lock actuator and S224. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
5 | Connect a test lamp between terminal 3 and ground. Does the test lamp illuminate with the door lock switch in the UNLOCK position? | Go to Step 7 | Go to Step 6
6 | Repair the open in the BLU/RED wire between the door lock actuator and S225. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 8 | --
7 | Replace the door lock actuator. Refer to Front Side Door Lock Actuator Replacement . Is the repair complete? | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3

## Power Door Locks Actuator Motor Inoperative Left Front

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Keyless Entry System Description , Keyless Entry System Operation and Keyless Entry System Circuit Description and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Doors
2 | Verify that the left front door lock is inoperative. Is only the left front door lock inoperative? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Disconnect the door lock actuator connector.
2. Connect a test lamp between terminal 2 and ground.

Does the test lamp illuminate with the door lock switch in the LOCK position?

Go to Step 5

Go to Step 4

4 | Repair the open in the BLU wire between the door lock actuator and S224. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 10 | --
5 | Connect a test lamp between terminal 3 and ground. Does the test lamp illuminate with the door lock switch in the UNLOCK position? | Go to Step 8 | Go to Step 6
6 |

1. Connect the door lock actuator connector.
2. Disconnect the remote control door lock receiver.
3. Ground terminal A of the remote control door lock receiver with a fused jumper wire.
4. Unlock the door.

Does the door lock when the door lock switch is in the LOCK position?

Go to Step 9

Go to Step 7

7 | Repair the open in the BLU/RED wire between the door lock actuator and the remote control door lock receiver. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to Step 10 | --
8 | Replace the door lock actuator. Refer to Front Side Door Lock Actuator Replacement . Is the repair complete? | Go to Step 10 | --
9 | Replace the remote control door lock receiver. Refer to Door Control Module Replacement . Is the repair complete? | Go to Step 10 | --
10 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3