For 1990-2009 cars

### Removal Procedure

1. Remove the heater case (1). Refer to Heater Case Replacement .
2. Remove 1 screw and heater core pipes bracket.
3. Remove the heater core (2) from the heater case (1).

### Installation Procedure

1. Install the heater core (2) to the heater case (1).
2. Install the heater core pipes bracket.
3. Secure the bracket with the 1 screw.
4. Install the heater case (1) to the vehicle. Refer to Heater Case Replacement .