For 1990-2009 cars

### Removal Procedure

1. Pull the rear seat lock handle.
2. Raise the rear seat cushion.
3. Remove the 3 plastic retainers which secure the front of the rear floor carpet (3).
4. Remove the 4 screws that secure the rear sill plate (4).
5. Remove the rear sill plate (4) from the vehicle.
6. Remove the rear floor carpet (3) from the vehicle.

### Installation Procedure

1. Install the rear floor carpet (3) to the vehicle.
2. Install the rear sill plate (4) to the vehicle. Secure the plate with the 4 screws.
3. Install the 3 plastic retainers to the front of the rear floor carpet.
4. Lower the rear seat cushion.