For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System Capacity 1.6 L Engine

- Engine, Radiator and Heater Core

4.6 Liters

5.0 Quarts

- Coolant Recovery Reservoir

0.9 Liters

0.8 Quarts

- Total

5.5 Liters

5.8 Quarts

Cooling System Capacity 2.0 L Engine

- Engine, Radiator and Heater Core

5.6 Liters

6.0 Quarts

- Coolant Recovery Reservoir

0.9 Liters

0.8 Quarts

- Total

6.5 Liters

6.8 Quarts

Coolant Solution Protection Point | -36°C | -33°F
Cooling System Pressure Capacity | 90 kPa | 13 psi
Generator/Coolant Pump Drive Belt Deflection | 5-8 mm at 10 kg applied pressure | 0.20-0.32 in at 22 lbs applied pressure
Radiator Cap Pressure Capacity | 90 kPa | 13 psi
Thermostat Valve Lift (Minimum) | 8 mm at 95°C | 0.31 in at 203°F
Thermostat Valve Opening Temperature | 80-90°C | 176-203°F