For 1990-2009 cars

1. Inspect the accelerator cable for proper adjustment. Refer to In Engine Controls.
2. Measure the distance between the tip end of the TV cable adjustment mark and the end of the boot. The distance must be 0.8-1.5 mm (0.031 -0.059 in).
3. Loosen the Throttle Control (TV) cable locknut (3) .
4. Adjust the cable using the locknuts until the measurement is achieved.
5. Tighten the TV cable locknut (3) .
6. Measure the distance between the tip end of the TV cable adjustment mark and the end of the boot. Ensure that the distance did not change during the tightening of the locknut.