For 1990-2009 cars

### J 38125-B Terminal Repair Kit

Use the J 38125-B Terminal Repair Kit for SIR wiring repair. This kit contains a special crimping tool, heat torch, and sealed splices. Do not use the terminals in the kit in order to replace damaged SIR system terminals unless specifically indicated by the terminal package.

### J 38826 SIR Deployment Harness

Use the J 38826 SIR Deployment Harness in order to deploy a driver inflator module outside of the vehicle. Use one of the following adapters in order to connect the deployment harness to the inflator module:

• | The J 38826-20 SIR Deployment Harness Adapter (pigtail connector)

• | The J 38826-50 SIR Deployment Harness Adapter (integral connector)

### J 38715-A SIR Driver/Passenger Load Tool

Use the J 38715-A SIR Driver/Passenger Load Tool only when the SIR diagnostics call for it. The Load Tool is used as a diagnostic aid and a safety device in order to prevent inadvertent inflator module deployment.

The load tool has four yellow connectors attached to its case. The three small connectors are electrically functional and serve as resistive load substitutions. The large dummy connector does not serve as a load substitution and is not used. Use no more than two connectors at any time.

One of the small connectors is used to substitute the load of the inflatable restraint steering wheel module. It is connected at the top of the column to the inflatable restraint steering wheel module coil. Use one of the following adapters to connect the load tool to the steering wheel module coil:

• | The J 38715-5 SIR Load Tool Adapter (pigtail connector)

• | The J 38715-30 Steering Column SIR Load Tool Adapter (integral connector)

A second small connector is used in order to substitute the load of the inflatable restraint steering wheel module and the inflatable restraint steering wheel module coil. The second small connector is connected at the base of the column to the SIR wiring harness. The third small connector is used to substitute for the load of the inflatable restraint IP module. The third small connector is connected to the inflatable restraint IP module harness connector.

Substitute the resistance of the inflator module in order to determine whether an inflator circuit component is causing a system malfunction. Use the load tool only when specifically called for in the diagnostic procedures.

### J 39200 Digital Multimeter

The J 39200 Digital Multimeter (DMM) is the preferred DMM for use in SIR diagnosis and repair. The J 34029-A may be used if the J 39200 is not available. No other DMMs are approved for SIR diagnosis and repair.

### J 35616-A Connector Test Adapter Kit

Use the J 35616-A Connector Test Adapter Kit whenever a diagnostic procedure requests checking or probing a terminal. Using the appropriate adapter will ensure that no damage to the terminal occurs from the DMM probe, such as spreading or bending. The adapter will also give an idea of whether contact tension is sufficient, helping to find an open or intermittent open due to poor terminal contact.

### J 39401-B SIR Deployment Fixture

Use the J39401B SIR Deployment Fixture when deploying passenger frontal air bags, side impact air bags, or seat belt pretensioners outside of the vehicle. Use the deployment fixture in order to secure the module for deployment.

### Scan Tool

The scan tool is used for the following reasons:

• | In order to read and clear SIR system Diagnostic Trouble Codes (DTCs)

• | In order to provide SIR system circuit values using the data list function

Refer to the scan tool operator's manual for specific information on how to use the scan tool.

### J 42113 Shorting Bar Tool

Use J 42113 Shorting Bar Tool only when the SIR diagnostics call for it. The shorting bar tool lifts any one of the shorting bars in the inflatable restraint sensing and diagnostic module (SDM) harness connector. When the shorting bar tool is installed into an SDM harness connector cavity to lift the shorting bar of an air bag loop, the shorting bridge to the air bag circuit is opened. When the shorting bar tool is installed into the SDM harness connector cavity to lift the shorting bar of AIR BAG warning lamp circuit, the AIR BAG warning lamp circuit is disconnected from the ground circuit, turning the AIR BAG warning lamp off.