For 1990-2009 cars

### Removal Procedure

1. Remove the ashtray and guide. Refer to Ashtray Replacement in Instrument Panel, Gauges and Console.
2. Remove the screw (2) which secures the IP ashtray lamp housing.
3. Position the ashtray lamp housing (1) as necessary in order to gain access to the ashtray lamp bulb.
4. Remove the ashtray lamp bulb from the housing (1).

### Installation Procedure

1. Install the ashtray lamp bulb to the ashtray lamp housing (1).
2. Install the ashtray lamp housing to the instrument panel. Secure the housing with the screw (2).
3. Install the ashtray and guide. Refer to Ashtray Replacement in Instrument Panel, Gauges and Console.