For 1990-2009 cars

## Door Lock and Side Window Switch Replacement Left Front

### Removal Procedure

1. Gently pry the left front side master window switch (1) from the front side door trim panel (4).
2. Disconnect the window switch and the door lock electrical connectors.
3. Remove the window switch (1) from the vehicle.

### Installation Procedure

1. Connect the left front side master window switch and the door lock electrical connectors.
2. Install the master window switch (1) to the front side door trim panel (4). Ensure that the retaining tabs are fully engaged.