For 1990-2009 cars

### Removal Procedure

1. Remove the front side door inside handle (2). Refer to Front Side Door Inside Handle Replacement .
2. Remove the outside rearview mirror opening cover (1).
3. Remove the screw which secures the front side door pull handle (3).
4. Gently pry the front side door trim panel (4) from the front side door by disengaging the plastic retainers which secure the panel.
5. Position the door trim panel (4) away from the door in order to gain access to the right front side window switch electrical connector.
6. Disconnect the window switch electrical connector.
7. Remove the door trim panel (4) from the vehicle.
8. Remove the front side window switch from the door trim panel (4) by releasing the 4 plastic retaining tabs.

### Installation Procedure

1. Install the right front side window switch to the front side door trim panel (4). Ensure that the 4 plastic retaining tabs are fully engaged.
2. Connect the front side window switch electrical connector.
3. Install the door trim panel (4) to the front side door. Ensure that the plastic retainers are fully engaged.
4. Install the screw which secures the front side door pull handle (3).
5. Install the outside rearview mirror opening cover (1).
6. Install the front side door inside handle (3). Refer to Front Side Door Inside Handle Replacement .