For 1990-2009 cars

### Removal Procedure

1. Push in the rear seat head restraint release button (2) and remove the rear seat head restraint (1) from the guides (3).
2. Use a flat-bladed tool in order to gently pry the seat head restraint guides (1) from the rear seat back cushion (2), if necessary.

### Installation Procedure

1. Install the rear seat head restraint guides (1) to the rear seat back cushion (2), if removed.
2. Push in the rear seat head restraint release button (2) and install the rear seat head restraint (1) to the guides (3).