For 1990-2009 cars

## Rear Door Trim Panel Replacement Lower

### Removal Procedure

Remove the rear door trim panel (4) from the rear door by gently prying loose the plastic retainers which secure the panel.

### Installation Procedure

Install the rear door trim panel (4) to the rear door. Ensure that the plastic retainers are fully engaged.

## Rear Door Trim Panel Replacement Upper Left

### Removal Procedure

1. Remove the high mounted stoplamp. Refer to High Mount Stop Lamp Replacement in Lighting Systems.
2. Remove the left rear door upper trim panel (3) from the rear door by gently prying loose the plastic retainers which secure the panel.

### Installation Procedure

1. Install the left rear door upper trim panel (3) to the rear door. Ensure that the plastic retainers are fully engaged.
2. Install the high mounted stoplamp. Refer to High Mount Stop Lamp Replacement in Lighting Systems.

## Rear Door Trim Panel Replacement Upper Right

### Removal Procedure

1. Remove the left rear door upper trim panel (3). Refer to Rear Door Trim Panel Replacement .
2. Gently pry the right rear door upper trim panel (1) from the rear door.
3. Remove the high mounted stoplamp wiring harness from the back of the upper trim panel (1).
4. Remove the rear door upper trim panel (1) from the vehicle.

### Installation Procedure

1. Install the high mounted stoplamp wiring harness to the back of the right rear door upper trim panel (1).
2. Install the right rear door upper trim panel (1) to the rear door. Ensure that the plastic retainers are fully engaged.
3. Install the left rear door upper trim panel (3). Refer to Rear Door Trim Panel Replacement .