For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
DEFINITION: All chimes appear to be inoperative.
1 | Did you review the audible warnings operation and perform the necessary inspections? | -- | Go to Step 2 | Go to Symptoms - Instrument Panel, Gages and Console
2 |

1. With the LF door open, insert the ignition key into the ignition switch.
2. With the seat belt unbuckled, turn ON the ignition.
3. With the LF door open, remove the key from the ignition and place the headlamp switch in the PARK position.

Did all of the chimes operate normally?

--

Go to Testing for Intermittent Conditions and Poor Connections

Go to Step 3

3 | Is the remainder of the instrument cluster operating normally? | -- | Go to Step 7 | Go to Step 4
4 | Test the ground circuit at terminal 10 of instrument cluster connector C2 for an open. Did you find and correct the condition? | -- | Go to Step 8 | Go to Step 5
5 | Test the ignition positive voltage circuit at terminal 14 of C1 for an open. Did you find and correct the condition? | -- | Go to Step 8 | Go to Step 6
6 | Repair/replace the instrument cluster printed circuit. Refer to Flat Wire Repairs in Wiring Systems or Printed Instrument Cluster Circuit Replacement . Did you complete the repair/replacement? | -- | Go to Step 8 | --
7 | Replace the multifunction alarm. Refer to Multifunction Alarm Module Replacement . Did you complete the replacement? | -- | Go to Step 8 | --
8 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 3