For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.
2. Remove 4 defroster air outlet screws.
3. Remove the defroster air outlet (3).
4. Remove the side defroster air outlets (2,4) from the defroster air outlet (3).

### Installation Procedure

1. Install the side defroster air outlets (2,4) to the defroster air outlet (3).
2. Install the defroster air outlet (3) and secure with the 4 screws.
3. Install the instrument panel. Refer to Instrument Panel Carrier Replacement in Instrument Panel, Gauges and Console.